|  |  |  |
| --- | --- | --- |
| **Specifications** | **DO110** | **DO180** |
| **Overall Dimensions** | 29 1/2"L x 24 1/4"W x 23"D | 41 1/2"L x 27"W x 36"H |
| **Chimney** | 7" I.D. Smoke Pipe | 8" I.D. Smoke Pipe |
| **Cast Iron Wood Fire Door** | 12" x 14" | 12 x 14" |
| **Water Capacity** | 31 US Gallons | 54 US Gallons |
| **Shipping Weight** | 510 lbs | 710 lbs |
| **Domestic Hot Water Coil** | Standard | Standard |
| **Round Firebox** | 20" Diameter x 23 1/4" Tall | 23 1/2" Diameter x 35" Tall |

|  |  |
| --- | --- |
| **Control Kits:** |  |
| Transformer (2) | Damper Motor |
| Normally Open Zone Valve | Triple Aquastat |
| 1/2" Drain Valve | Pressure Relief Valve |
| 1 1/4" Supply/Return (Connections) | Tridicator |
|  | Interlock Relay |

|  |
| --- |
| **Indoor Wood Fired Boiler and Furnace** |
| The “Dutch Oven” concept of completely surrounding the firebox with cooling water prevents damage from overheating and eliminates the need for firebrick.   * This boiler is made of steel plate for long life * Domestic hot water coil included * Designed for use as an add-on to the primary heating source * No messy firetubes to clean * Compact size uses less of your valuable floor space * With proper installation, the unit may be used as a gravity unit during a power failure * 6 year limited warranty   This furnace is certified to be installed either by itself (with optional blower) or in conjunction with an existing warm air furnace. Firebox size is 22”x29-1/3” and an optional blower can be mounted on either side of unit.   * Specifications: • Overall Dimensions: 34”L x 28”W x 43”H • Shipping Weight: 360 lbs • Warm Air Plenum: 24”x30” • 7” I.D. Smoke Pipe • 2”x14” Cast Iron Wood Fire Door • 6 Year Limited Warranty   Control Kit:   * Damper Motor * J-Box / Cover * Transformer * Fan Limit c/w bracket * Thermostat   ***Call Us TOLL FREE: 1-888-385-HEAT (4328)*** |

|  |  |
| --- | --- |
|  |  |