**Detailed Request for Permit**

**Basement**

In the hallway between Bathrooms 1&2 and the closet under the stairs

1. New 2/4 fire wall 5/8 fire code sheetrock on both sides with 3’0”X 6’8” 1hour fire rated door with self closing hinges.
2. New 1 hour fire rated door on the left of the boiler room.

**First floor**

Repair the outside back porch on the left

1. Replace (24) 3”x5” decorative rafters 2’ on center fastened with joist hangers.
2. Replace (2x8) ledger against the wall fastened with 3 1/2” anchors in between ea. Rafter.

Media Office

1. New 2/4 wall with 5/8 fire code sheetrock on both sides with 3’0”X 6’8”

1 hour fire rated door with self closing hinges

1. Replace wood door on the right going to the basement with a 1 hour fire rated door with metal frame and self closing hinges.
2. Replace wood doors at the bottom of the stairs on the left and right going to the Learning Center with 1 hour fire rated 3’0”X 6’8” doors with metal frames and overhead closures.
3. Replace exterior back door by small porch with a 3’0”X 6’8” decorative wood door, metal frame and crash bar with overhead closure.

Sitting Room #1

1. Replace wood door on the left with a 1 hour fire rated 3’0”X 6’8” door with metal frame and overhead closure.

Main hallway

1. Replace exterior back wood door with a 3’0”X 6’8” decorative wood door, metal frame and crash bar with overhead closure.
2. Replace basement door at the top of the stairs on the right with 1 hour fire rated 3’0”X 6’8” door with metal frame and self closing hinges.
3. In the center of the Main hallway replace wood door with a 1 hour fire rated 3’0”X 6’8” door with metal frame and overhead closure.
4. Replace sitting room # 2 wood door at the bottom of the stairs on the left with 1 hour fire rated 3’0”X 6’8” door with metal frame and self closing hinges.
5. Replace nursery wood door at the bottom of the stairs on the right with 1 hour fire rated 3’0”X 6’8” door with metal frame and self closing hinges.
6. In the hallway between the nursery and the#2 sitting room

New 2/4 wall with 5/8 fire code sheetrock on both sides with 3’0”X 6’8”

1 hour fire rated door with overhead closure.

**Second Floor**

1. Storage #1 replace wood door with 2’8” x 6’8” 20 min fire rated door with self closing hinges
2. Bed room #1 replace wood door with 2’8” x 6’8” 20 min fire rated door with self closing hinges.
3. Bed room #2 replace wood door with 3’0” x 6’8” 20 min fire rated door with self closing hinges.
4. Bed room #3 replace wood door with 3’0” x 6’8” 20 min fire rated door with self closing hinges.
5. By room #3 at the bottom of the stairs to the third floor, install a 2x4 wall with 5/8 fire code sheetrock and a 2’8’x6’8” 1 hour fire rated door with self closing hinges, and a 2x4 wall with 5/8 fire code sheetrock on both sides along side of the 3rd floor and fourth floor stairwells, all the way across to the #3 storage room.
6. Bed room #4 replace wood door with 3’0” x 6’8” 20 min fire rated door with self closing hinges.
7. Bed room #5 replace wood door with 3’0” x 6’8” 20 min fire rated door with self closing hinges.
8. In the center of the hallway replace wood door with a 1 hour fire rated 3’0”X 6’8” door with metal frame and overhead closure.
9. In the hallway between bedroom #2 and bedroom #5

Install a New 2/4 wall with 5/8 fire code sheetrock on both sides with 3’0”X 6’8”

1 hour fire rated door with overhead closure.

1. Bed room #6 replace wood door with 2’8” x 6’8” 20 min fire rated door with self closing hinges.
2. Bed room #7 replace wood door with 2’8” x 6’8” 20 min fire rated door with self closing hinges.
3. Bed room #8 replace wood door with 2’8” x 6’8” 20 min fire rated door with self closing hinges.
4. In the center of the Hallway by bedroom # 8 install a New 2x4 wall with 5/8 fire code sheetrock, a 3’0”x6’8” 1 hour fire rated door with overhead closure.

**Third Floor**

1. Storage #1 replace door, 2’8” x 6’8” 20 min fire rated door with self closing hinges.