|  |  |  |  |
| --- | --- | --- | --- |
| **Model** |  | WC100 | WC200 |
| **Outside Dimensions** | Height \* | 46.5" | 52.5" |
|  | Width | 26.5" | 26.5" |
|  | Length \*\* | 24.5" | 33.5" |
|  | Shipping Weight | 687 lbs. | 947 lbs. |
| **Firebox Dimensions** | Height | 21" | 25" |
|  | Width | 18" | 18" |
|  | Length | 20" | 29" |
| **Door Size** | Height | 13" | 16" |
|  | Width | 13" | 16" |
|  |  |  |  |
| Log Length |  | 18" | 27" |
| **Flue** |  | 6" diameter | 7" diameter |
| **BTU's / hr \*\*\*** |  | 100,00 | 200,000 |
| **Gallons** |  | 24 | 40 |

|  |
| --- |
| **WC100/WC200 Wood/Coal Fired Boilers** |
| The Wasser Boiler is designed to be installed in your basement, garage, or shop. The shaker grate combustion chamber with secondary air ensures the high efficiency combustion of wood and/or coal.   * Features: -Shaker grate for easier and cleaner maintenance -Ash pan with separate door -Large firebox door for easy fueling -Optional electric back up   **Specifications:**  **Standard Features (WC100 & WC200):**   * Shaker Grates * Ash Pan * Automatic Temperature Control * Over Temperature Control * Temperature/Pressure Gauge * Fire Brick Lined   **Options**   * Electric Backup   ***Call Us TOLL FREE: 1-888-385-HEAT (4328)*** |